   IANAifType-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       MODULE-IDENTITY, mib-2      FROM SNMPv2-SMI
       TEXTUAL-CONVENTION          FROM SNMPv2-TC;

   ianaifType MODULE-IDENTITY
       LAST-UPDATED "200105110000Z"  -- May 11, 2001
       ORGANIZATION "IANA"
       CONTACT-INFO "        Internet Assigned Numbers Authority

                     Postal: ICANN
                             4676 Admiralty Way, Suite 330
                             Marina del Rey, CA 90292

                     Tel:    +1 310 823 9358
                     E-Mail: iana@iana.org"
       DESCRIPTION  "This MIB module defines the IANAifType Textual
                     Convention, and thus the enumerated values of
                     the ifType object defined in MIB-II's ifTable."

       REVISION     "200105110000Z"  -- May 11, 2001
       DESCRIPTION  "Registration of new IANAifType
                    197."

       REVISION     "200101120000Z"  -- Jan 12, 2001
       DESCRIPTION  "Registration of new IANAifTypes
                    195 and 196."

       REVISION     "200012190000Z"  -- Dec 19, 2000
       DESCRIPTION  "Registration of new IANAifTypes
                    193 and 194."

       REVISION     "200012070000Z"  -- Dec 07, 2000
       DESCRIPTION  "Registration of new IANAifTypes
                    191 and 192."

       REVISION     "200012040000Z"  -- Dec 04, 2000
       DESCRIPTION  "Registration of new IANAifType
                    190."

       REVISION     "200010170000Z"  -- Oct 17, 2000
       DESCRIPTION  "Registration of new IANAifTypes
                    188 and 189."  

       REVISION     "200010020000Z"  -- Oct 02, 2000
       DESCRIPTION  "Registration of new IANAifType 187." 

       REVISION     "200009010000Z"  -- Sept 01, 2000
       DESCRIPTION  "Registration of new IANAifTypes
                     184, 185, and 186."			

       REVISION     "200008240000Z"  -- Aug 24, 2000
       DESCRIPTION  "Registration of new IANAifType 183." 

       REVISION     "200008230000Z"  -- Aug 23, 2000
       DESCRIPTION  "Registration of new IANAifTypes
                     174-182."

       REVISION     "200008220000Z"  -- Aug 22, 2000
       DESCRIPTION  "Registration of new IANAifTypes 170,
                     171, 172 and 173."

       REVISION     "200004250000Z"  -- Apr 25, 2000
       DESCRIPTION  "Registration of new IANAifTypes 168 and 169."       

       REVISION     "200003060000Z"  -- Mar 6, 2000
       DESCRIPTION  "Fixed a missing semi-colon in the IMPORT.
                     Also cleaned up the REVISION log a bit.
                     It is not complete, but from now on it will
                     be maintained and kept up to date with each
                     change to this MIB module."

       REVISION     "199910081430Z"  -- Oct 08, 1999
       DESCRIPTION  "Include new name assignments up to cnr(85).
                     This is the first version available via the WWW
                     at: ftp://ftp.isi.edu/mib/ianaiftype.mib"

       REVISION     "199401310000Z"  -- Jan 31, 1994
       DESCRIPTION  "Initial version of this MIB as published in
                     RFC 1573."
       ::= { mib-2 30 }

   IANAifType ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
               "This data type is used as the syntax of the ifType
               object in the (updated) definition of MIB-II's
               ifTable.

               The definition of this textual convention with the
               addition of newly assigned values is published
               periodically by the IANA, in either the Assigned
               Numbers RFC, or some derivative of it specific to
               Internet Network Management number assignments.  (The
               latest arrangements can be obtained by contacting the
               IANA.)

               Requests for new values should be made to IANA via
               email (iana@iana.org).

               The relationship between the assignment of ifType
               values and of OIDs to particular media-specific MIBs
               is solely the purview of IANA and is subject to change
               without notice.  Quite often, a media-specific MIB's
               OID-subtree assignment within MIB-II's 'transmission'
               subtree will be the same as its ifType value.
               However, in some circumstances this will not be the
               case, and implementors must not pre-assume any
               specific relationship between ifType values and
               transmission subtree OIDs."
       SYNTAX  INTEGER {
                   other(1),          -- none of the following
                   regular1822(2),
                   hdh1822(3),
                   ddnX25(4),
                   rfc877x25(5),
                   ethernetCsmacd(6),
                   iso88023Csmacd(7),
                   iso88024TokenBus(8),
                   iso88025TokenRing(9),
                   iso88026Man(10),
                   starLan(11),
                   proteon10Mbit(12),
                   proteon80Mbit(13),
                   hyperchannel(14),
                   fddi(15),
                   lapb(16),
                   sdlc(17),
                   ds1(18),            -- DS1-MIB
                   e1(19),             -- Obsolete see DS1-MIB
                   basicISDN(20),
                   primaryISDN(21),
                   propPointToPointSerial(22), -- proprietary serial
                   ppp(23),
                   softwareLoopback(24),
                   eon(25),            -- CLNP over IP 
                   ethernet3Mbit(26),
                   nsip(27),           -- XNS over IP
                   slip(28),           -- generic SLIP
                   ultra(29),          -- ULTRA technologies
                   ds3(30),            -- DS3-MIB
                   sip(31),            -- SMDS, coffee
                   frameRelay(32),     -- DTE only. 
                   rs232(33),
                   para(34),           -- parallel-port
                   arcnet(35),         -- arcnet
                   arcnetPlus(36),     -- arcnet plus
                   atm(37),            -- ATM cells
                   miox25(38),
                   sonet(39),          -- SONET or SDH 
                   x25ple(40),
                   iso88022llc(41),
                   localTalk(42),
                   smdsDxi(43),
                   frameRelayService(44),  -- FRNETSERV-MIB
                   v35(45),
                   hssi(46),
                   hippi(47),
                   modem(48),          -- Generic modem
                   aal5(49),           -- AAL5 over ATM
                   sonetPath(50),
                   sonetVT(51),
                   smdsIcip(52),       -- SMDS InterCarrier Interface
                   propVirtual(53),    -- proprietary virtual/internal
                   propMultiplexor(54),-- proprietary multiplexing
                   ieee80212(55),      -- 100BaseVG
                   fibreChannel(56),   -- Fibre Channel
                   hippiInterface(57), -- HIPPI interfaces     
                   frameRelayInterconnect(58), -- Obsolete use either
                                       -- frameRelay(32) or 
                                       -- frameRelayService(44).
                   aflane8023(59),     -- ATM Emulated LAN for 802.3
                   aflane8025(60),     -- ATM Emulated LAN for 802.5
                   cctEmul(61),        -- ATM Emulated circuit          
                   fastEther(62),      -- Fast Ethernet (100BaseT)
                   isdn(63),           -- ISDN and X.25           
                   v11(64),            -- CCITT V.11/X.21             
                   v36(65),            -- CCITT V.36                  
                   g703at64k(66),      -- CCITT G703 at 64Kbps
                   g703at2mb(67),      -- Obsolete see DS1-MIB
                   qllc(68),           -- SNA QLLC                    
                   fastEtherFX(69),    -- Fast Ethernet (100BaseFX)   
                   channel(70),        -- channel                     
                   ieee80211(71),      -- radio spread spectrum       
	           ibm370parChan(72),  -- IBM System 360/370 OEMI Channel
                   escon(73),          -- IBM Enterprise Systems Connection
                   dlsw(74),           -- Data Link Switching
                   isdns(75),          -- ISDN S/T interface
                   isdnu(76),          -- ISDN U interface
                   lapd(77),           -- Link Access Protocol D
                   ipSwitch(78),       -- IP Switching Objects
                   rsrb(79),           -- Remote Source Route Bridging
                   atmLogical(80),     -- ATM Logical Port
                   ds0(81),            -- Digital Signal Level 0
                   ds0Bundle(82),      -- group of ds0s on the same ds1
                   bsc(83),            -- Bisynchronous Protocol
                   async(84),          -- Asynchronous Protocol
                   cnr(85),            -- Combat Net Radio
                   iso88025Dtr(86),    -- ISO 802.5r DTR
                   eplrs(87),          -- Ext Pos Loc Report Sys
                   arap(88),           -- Appletalk Remote Access Protocol
                   propCnls(89),       -- Proprietary Connectionless Protocol
                   hostPad(90),        -- CCITT-ITU X.29 PAD Protocol
                   termPad(91),        -- CCITT-ITU X.3 PAD Facility
                   frameRelayMPI(92),  -- Multiproto Interconnect over FR
                   x213(93),           -- CCITT-ITU X213
                   adsl(94),           -- Asymmetric Digital Subscriber Loop
                   radsl(95),          -- Rate-Adapt. Digital Subscriber Loop
                   sdsl(96),           -- Symmetric Digital Subscriber Loop
                   vdsl(97),           -- Very H-Speed Digital Subscrib. Loop
                   iso88025CRFPInt(98), -- ISO 802.5 CRFP
                   myrinet(99),        -- Myricom Myrinet
                   voiceEM(100),       -- voice recEive and transMit
                   voiceFXO(101),      -- voice Foreign Exchange Office
                   voiceFXS(102),      -- voice Foreign Exchange Station
                   voiceEncap(103),    -- voice encapsulation
                   voiceOverIp(104),   -- voice over IP encapsulation
                   atmDxi(105),        -- ATM DXI
                   atmFuni(106),       -- ATM FUNI
		   atmIma (107),       -- ATM IMA		   
                   pppMultilinkBundle(108), -- PPP Multilink Bundle
                   ipOverCdlc (109),   -- IBM ipOverCdlc
		   ipOverClaw (110),   -- IBM Common Link Access to Workstn
                   stackToStack (111), -- IBM stackToStack
                   virtualIpAddress (112), -- IBM VIPA
		   mpc (113),          -- IBM multi-protocol channel support
		   ipOverAtm (114),    -- IBM ipOverAtm
		   iso88025Fiber (115), -- ISO 802.5j Fiber Token Ring
		   tdlc (116),	       -- IBM twinaxial data link control
		   gigabitEthernet (117), -- Gigabit Ethernet
		   hdlc (118),         -- HDLC
		   lapf (119),	       -- LAP F
		   v37 (120),	       -- V.37
		   x25mlp (121),       -- Multi-Link Protocol
		   x25huntGroup (122), -- X25 Hunt Group
		   trasnpHdlc (123),   -- Transp HDLC
		   interleave (124),   -- Interleave channel
		   fast (125),         -- Fast channel
		   ip (126),	       -- IP (for APPN HPR in IP networks)
		   docsCableMaclayer (127),  -- CATV Mac Layer
		   docsCableDownstream (128), -- CATV Downstream interface
		   docsCableUpstream (129),  -- CATV Upstream interface
		   a12MppSwitch (130), -- Avalon Parallel Processor
		   tunnel (131),       -- Encapsulation interface
		   coffee (132),       -- coffee pot
		   ces (133),          -- Circuit Emulation Service
		   atmSubInterface (134), -- ATM Sub Interface
		   l2vlan (135),       -- Layer 2 Virtual LAN using 802.1Q
		   l3ipvlan (136),     -- Layer 3 Virtual LAN using IP
		   l3ipxvlan (137),    -- Layer 3 Virtual LAN using IPX
		   digitalPowerline (138), -- IP over Power Lines	
		   mediaMailOverIp (139), -- Multimedia Mail over IP
		   dtm (140),        -- Dynamic syncronous Transfer Mode
		   dcn (141),    -- Data Communications Network
		   ipForward (142),    -- IP Forwarding Interface
		   msdsl (143),       -- Multi-rate Symmetric DSL
		   ieee1394 (144), -- IEEE1394 High Performance Serial Bus
		   if-gsn (145),       --   HIPPI-6400 
		   dvbRccMacLayer (146), -- DVB-RCC MAC Layer
		   dvbRccDownstream (147),  -- DVB-RCC Downstream Channel
		   dvbRccUpstream (148),  -- DVB-RCC Upstream Channel
		   atmVirtual (149),   -- ATM Virtual Interface
		   mplsTunnel (150),   -- MPLS Tunnel Virtual Interface
		   srp (151),	-- Spatial Reuse Protocol	
		   voiceOverAtm (152),  -- Voice Over ATM
		   voiceOverFrameRelay (153),   -- Voice Over Frame Relay 
		   idsl (154),		-- Digital Subscriber Loop over ISDN
		   compositeLink (155),  -- Avici Composite Link Interface
		   ss7SigLink (156),     -- SS7 Signaling Link 
		   propWirelessP2P (157),  --  Prop. P2P wireless interface
		   frForward (158),    -- Frame Forward Interface
		   rfc1483 (159),	-- Multiprotocol over ATM AAL5
		   usb (160),		-- USB Interface
		   ieee8023adLag (161),  -- IEEE 802.3ad Link Aggregate
                   bgppolicyaccounting (162), -- BGP Policy Accounting
                   frf16MfrBundle (163), -- FRF .16 Multilink Frame Relay 
                   h323Gatekeeper (164), -- H323 Gatekeeper
                   h323Proxy (165), -- H323 Voice and Video Proxy
                   mpls (166), -- MPLS                   
                   mfSigLink (167), -- Multi-frequency signaling link
                   hdsl2 (168), -- High Bit-Rate DSL - 2nd generation
                   shdsl (169), -- Multirate HDSL2
                   ds1FDL (170), -- Facility Data Link 4Kbps on a DS1
                   pos (171), -- Packet over SONET/SDH Interface
                   dvbAsiIn (172), -- DVB-ASI Input
                   dvbAsiOut (173), -- DVB-ASI Output 
                   plc (174), -- Power Line Communtications
                   nfas (175), -- Non Facility Associated Signaling
                   tr008 (176), -- TR008
                   gr303RDT (177), -- Remote Digital Terminal
                   gr303IDT (178), -- Integrated Digital Terminal
                   isup (179), -- ISUP
                   propDocsWirelessMaclayer (180), -- prop/Maclayer
                   propDocsWirelessDownstream (181), -- prop/Downstream
                   propDocsWirelessUpstream (182), -- prop/Upstream
                   hiperlan2 (183), -- HIPERLAN Type 2 Radio Interface
                   propBWAp2Mp (184), -- PropBroadbandWirelessAccesspt2multipt
                   sonetOverheadChannel (185), -- SONET Overhead Channel
                   digitalWrapperOverheadChannel (186), -- Digital Wrapper
                   aal2 (187), -- ATM adaptation layer 2
                   radioMAC (188), -- MAC layer over radio links
                   atmRadio (189), -- ATM over radio links   
                   imt (190), -- Inter Machine Trunks
                   mvl (191), -- Multiple Virtual Lines DSL
                   reachDSL (192), -- Long Reach DSL
                   frDlciEndPt (193), -- Frame Relay DLCI End Point
                   atmVciEndPt (194), -- ATM VCI End Point
                   opticalChannel (195), -- Optical Channel
                   opticalTransport (196), -- Optical Transport
                   propAtm (197) -- Proprietary ATM
}

   END
